# **RG Android Device Upgrade the firmware** (via SD card)

## **Introduction**

This article mainly introduced how to upgrade the firmware on the host to the SD card, which needs to be selected according to the host operating system.

## **Preparatory Tools**

RGxxx DeviceFirmware host computer USB Card Reader MIrcoSD card [SD\_Firmware\_Tool](http://en.t-firefly.com/doc/download/93.html" \l "other_368)


## **Operation Steps**

Insert microSD card into USB card reader and then into USB port of host computer

Run SD\_Firmware\_Tool, check the “Upgrade Firmware” box and select the correct removable disk device

Choose firmware we want to upgrade into the RGxxx device

Click button <Create> to make it and wait until it is finshed



Remove the microSD card, insert it into the microSD card slot of the motherboard, power on the board, it will start upgrading automatically.it will start upgrading automatically.This process takes ten minutes

After the upgrade, remove the microSD card and restart the motherboard automatically to complete the whole process of firmware update

It takes some time to boot up for the first time, enter the desktop and wait for a while to complete the configuration of the phone boot, and then you can enjoy the handheld